## Configuration

|  |  |  |
| --- | --- | --- |
|  | TypeWall | TypeRoof |
| OnlyVCWG | SteelFrame  Emissivity: 0.9  Albedo: 0.5 | IEAD  Emissivity: 0.94  Albedo: 0.5 |
| Bypass | Steel Frame Non-res Ext Wall  Thermal absorptance: 0.9  Solar absorptance: 0.5  Visible absorptance: 0.5 | IEAD Non-res Roof  Thermal absorptance: 0.94  Solar absorptance: 0.5  Visible absorptance: 0.5 |

## Performance

CVRMSE (%), (OnlyEP, OnlyVCWG, Bypass)

2m, direct: [ 7.32 17.44 18.24]

2m, real\_p0: [ nan 18.64 19.53]

2m, real\_epw: [ nan 15.97 16.64]

6m, direct: [ 7.32 16.51 17.04]

6m, real\_p0: [ nan 17.51 18.13]

6m, real\_epw: [ nan 15.02 15.37]

20m, direct: [ 6.29 17.59 16.91]

20m, real\_p0: [ nan 18.02 17.42]

20m, real\_epw: [ nan 16.18 15.21]Chart, histogram

Description automatically generated